*LIGO Laboratory / LIGO Scientific Collaboration*

LIGO- E1100962-v1 *Advanced LIGO* 30 September 2011

Test Procedure for the Picomotor Feedthrough and Breakout

Daniel Sigg

Distribution of this document:

LIGO Scientific Collaboration

This is an internal working note

of the LIGO Laboratory.

|  |  |
| --- | --- |
| **California Institute of Technology****LIGO Project – MS 18-34****1200 E. California Blvd.****Pasadena, CA 91125**Phone (626) 395-2129Fax (626) 304-9834E-mail: info@ligo.caltech.edu | **Massachusetts Institute of Technology****LIGO Project – NW22-295****185 Albany St****Cambridge, MA 02139**Phone (617) 253-4824Fax (617) 253-7014E-mail: info@ligo.mit.edu |
| **LIGO Hanford Observatory****P.O. Box 1970****Richland WA 99352**Phone 509-372-8106Fax 509-372-8137 | **LIGO Livingston Observatory****P.O. Box 940****Livingston, LA 70754**Phone 225-686-3100Fax 225-686-7189 |

http://www.ligo.caltech.edu/

# Overview

The picomotor feedthrough, [D1101691-v1](https://dcc.ligo.org/public/0069/D1101691/001/D1101691-v1.pdf), connects to the front panel of a picomotor controller, [D1100323-v2](https://dcc.ligo.org/public/0039/D1100323/002/D1100323-v2.pdf), using a DB25 cable. The 2 DB9 outputs connect to a picomotor breakout box, [D1101738-v2](https://dcc.ligo.org/public/0069/D1101738/002/D1101738-v2.pdf), which contains 4 RJ-11 sockets to connect to 4 different picomotor axes. The picomotor controller is connected to a EtherCAT/Beckhoff system. The test software is described in [T1100458-v1](https://dcc.ligo.org/public/0069/T1100458/001/T1100458-v1.pdf).

# Test Equipment

* Picomotor controller, [D1100323-v2](https://dcc.ligo.org/public/0039/D1100323/002/D1100323-v2.pdf).
* Computer with EtherCAT/Beckhoff software for controlling picomotors.
* 1 DB25 m-f cable.
* 2 DB9 m-f cable.
* 1 picomotor with RJ-11 connector.
* DC power supplies.

# Feedthrough Test

Power up the measurement equipment and connect the picomotor feedthrough (DUT) as well as 1 or 2 picomotor breakout boxes. Connect the picomotor to the first axis and use the computer to drive it. Continue this for all 8 axes.

|  |  |  |
| --- | --- | --- |
| **Breakout** | **Axes** | **Pass/Fail** |
| 1 | 1X |  |
| 1 | 1Y |  |
| 1 | 2X |  |
| 1 | 2Y |  |
| 2 | 1X |  |
| 2 | 1Y |  |
| 2 | 2X |  |
| 2 | 2Y |  |

# Breakout Box Test

Power up the measurement equipment and connect a picomotor feedthrough as well as the picomotor breakout box (DUT). Connect the picomotor to the first axis and use the computer to drive it. Continue this for all 4 axes.

|  |  |
| --- | --- |
| **Axes** | **Pass/Fail** |
| 1X |  |
| 1Y |  |
| 2X |  |
| 2Y |  |