*LIGO Laboratory / LIGO Scientific Collaboration*

LIGO- E1200627-v2 Advanced LIGO 9/4/2013

TwinCAT Library for   
Delay Line

Alexa Staley, Daniel Sigg

Distribution of this document:

LIGO Scientific Collaboration

This is an internal working note  
of the LIGO Laboratory.

|  |  |
| --- | --- |
| **California Institute of Technology**  **LIGO Project – MS 18-34**  **1200 E. California Blvd.**  **Pasadena, CA 91125**  Phone (626) 395-2129  Fax (626) 304-9834  E-mail: info@ligo.caltech.edu | **Massachusetts Institute of Technology**  **LIGO Project – NW22-295**  **185 Albany St**  **Cambridge, MA 02139**  Phone (617) 253-4824  Fax (617) 253-7014  E-mail: info@ligo.mit.edu |
| **LIGO Hanford Observatory**  **P.O. Box 159**  **Richland WA 99352**  Phone 509-372-8106  Fax 509-372-8137 | **LIGO Livingston Observatory**  **P.O. Box 940**  **Livingston, LA 70754**  Phone 225-686-3100  Fax 225-686-7189 |

http://www.ligo.caltech.edu/

|  |  |
| --- | --- |
| **Library** | |
| Title | DelayLinePhaseShifter |
| Version | 1 |
| TwinCAT version | 2.11 |
| Name space | – |
| Author | Alexa Staley, Daniel Sigg |
| Description | The delay line shifter delays an input signal by a selectable amount. This amount can be controlled by a step or phase slider. The delay can be between 0ns and 30.762ns. |
| Error Codes | 0x01 – Invalid frequency |
| Library dependencies | Error |

|  |  |
| --- | --- |
| **Hardware Output Type**  TYPE DelayLogicOutStruct :  STRUCT  DelayStep: INT;  LacthEn: BOOL;  END\_STRUCT  END\_TYPE | |
| Type name | DelayLogicOutStruct |
| Description | Structure of the hardware output that are wired up for the delay line |
| Definition | STRUCT |
| Element | Name: DelayStep  Type: INT  Description: The delay line step slider |
| Element | Name: LatchEn  Type: BOOL  Description: Enables latch |

|  |  |
| --- | --- |
| **User Interface Type**  TYPE DelayLogicStruct :  STRUCT  FreqMhz: LREAL;  PhaseDeg: LREAL;  DelayNs: LREAL;  DelayStep: INT;  Error: ErrorStruct;  END\_STRUCT  END\_TYPE | |
| Type name | DelayLogicStruct |
| Description | Structure of the user interface tags that are used to control the delay line |
| Definition | STRUCT |
| Output Tag | Name: Error  Type: ErrorStruct  Description: For error handling |
| Input Tag | Name: FreqMhz  Type: LREAL  Description: Input frequency in MHz |
| In/out Tag | Name: PhaseDeg  Type: LREAL  Description: Input phase in degrees |
| In/out Tag | Name: DelayNs  Type: LREAL  Description: Delay of input signal in nanoseconds |
| In/out Tag | Name: DelayStep  Type: INT  Description: Delay between 0ns and 31.9375ns can be added in steps |

|  |  |
| --- | --- |
| **Function Block**  FUNCTION\_BLOCK DelayLogicFB  VAR\_INPUT  Request: SaveRestoreEnum;  END\_VAR  VAR\_OUTPUT  DelayLogicOut: DelayLogicOutStruct;  END\_VAR  VAR\_IN\_OUT  DelayLogicInit: DelayLogicStruct;  DelayLogic: DelayLogicStruct;  END\_VAR | |
| Name | DelayLogicFB |
| Description | Controls the delay line |
| Input argument | Name: Request  Type: SaveRestoreEnum  Description: Request save/restore/safemode or noop |
| Output argument | Name: DelayLogicOut  Type: DelayLogicOutStruct  Description: Output hardware structure |
| In/out argument | Name: DelayLogicInit  Type: DelayLogicStruct  Description: Save/restore variable in persistent memory |
| In/out argument | Name: DelayLogic  Type: DelayLogicStruct  Description: User Interface structure |

|  |  |
| --- | --- |
| **Visual** | |
| Name | DelayLogicVis |
| Description | Displays phase, steps, and delay |
| Placeholder | Name: DelayLogic  Type: DelayLogicStruct  Description: Delay Line structure |