*LIGO Laboratory / LIGO Scientific Collaboration*

LIGO- E1100285 *LIGO* October 31, 2013

**aLIGO HEPI Control Implementation Procedure**

E1300825

Fabrice Matichard, Sebastien Biscans for the SEI Team

Distribution of this document:

Advanced LIGO Project

This is an internal working note

of the LIGO Laboratory

|  |  |
| --- | --- |
| **California Institute of Technology****LIGO Project – MS 18-34****1200 E. California Blvd.****Pasadena, CA 91125**Phone (626) 395-2129Fax (626) 304-9834E-mail: info@ligo.caltech.edu | **Massachusetts Institute of Technology****LIGO Project – NW22-295****185 Albany St****Cambridge, MA 02139**Phone (617) 253-4824Fax (617) 253-7014E-mail: info@ligo.mit.edu |
| **LIGO Hanford Observatory****P.O. Box 1970****Mail Stop S9-02****Richland WA 99352**Phone 509-372-8106Fax 509-372-8137 | **LIGO Livingston Observatory****P.O. Box 940****Livingston, LA 70754**Phone 225-686-3100Fax 225-686-7189 |

Contents

Contents 2

Control validation 4

1.1 Blend Filters 4

1.2 Isolation Loops 5

1.3 Sensor Correction 6

Introduction

# Control validation

## Blend Filters

The blend filters presented below were designed by Richard Mittleman for LASTI. The goal is to obtain a good compromise between noise injection and common rejection at low frequencies.

As an example, only one direction is plotted in this report.

**The filter is commited in the SVN at:**

/SeiSVN/seismic/HEPI/M1/HAMX/Scripts/Control\_Scripts/release/HEPI\_Blend\_Filters\_020713.mat

**Scripts files for processing and plotting in SVN at:**

/SeiSVN/seismic/HEPI/M1/HAMX/Scripts/Control\_Scripts/release/

* Step\_5\_Blend\_Filters\_M1\_HEPI\_HAMX.m

 **Figures in SVN at:**

/SeiSVN/seismic/HEPI/M1/HAMX/Data/ Figures/Transfer\_Functions/Simulations/Super\_Sensors/

* M1\_HPI\_HAMX\_Super\_Sensor\_SISO\_X\_Blend\_Freq\_0.46Hz.fig
* M1\_HPI\_HAMX\_Super\_Sensor\_MIMO\_X\_Blend\_Freq\_0.46Hz.fig

**Storage of measured transfer functions in the SVN at:**

/SeiSVN/seismic/HEPI/M1/HAMX/Data/Transfer\_functions/ Simulations/Super\_Sensors/

* M1\_HPI\_HAMX\_TF\_C2C\_SS\_Blend\_03\_2013p.mat





## Isolation Loops

Those isolation filters (level 2 UGF ~25 Hz) were designed by Rich Mitttleman and have been used at LASTI.

As an example, only one direction is plotted in this report.

**Scripts files for processing and plotting in SVN at:**

/SeiSVN/seismic/HEPI/M1/HAMX/Scripts/Control\_Scripts/release/

* Step\_6\_Isolation\_Filters\_Z\_RX\_RY\_VP\_M1\_HEPI\_HAMX.m
* Step\_7\_Isolation\_Filters\_X\_Y\_RZ\_HP\_M1\_HEPI\_HAMX.m
* Step\_8\_Loading\_Sensor\_Correction\_Filters\_M1\_HEPI\_HAMX.m

 **Figures in SVN at:**

/SeiSVN/seismic/HEPI/M1/HAMX/Data/ Figures/Transfer\_Functions/Simulations/Super\_Sensors/

* M1\_HPI\_HAMX\_Isolation\_Loops\_TF\_SISO\_ACT\_VP\_to\_SS\_VP\_03\_2013p.fig
* M1\_HPI\_HAMX\_Isolation\_Loops\_TF\_MIMO\_ACT\_VP\_to\_SS\_VP\_03\_2013p.fig

**Storage of measured transfer functions in the SVN at:**

/SeiSVN/seismic/HEPI/M1/HAMX/Data/Transfer\_functions/ Simulations/Super\_Sensors/

* M1\_HPI\_HAMX\_TF\_C2C\_Isolation\_V\_H\_Level\_1\_Blend\_testmHz\_03\_2013p.mat

## Sensor Correction

Procedure:

* Commissioning Scripts
* Validation Scripts

Appendix A

Housing Centering Procedure